AXUV array 1 (with horizontal resolution on plasma column; located at bottom flange)

Channel number | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16
r [mm] | -89.8 (-90.2) | -80.1 | -69.6 | -58.7 | -47.5 | -35.9 | -24.2 | -12.2 | -0.1 | 12.0 | 24.1 | 36.1 | 47.9 | 59.4 | 70.7 | 81.6
a [deg] | 21.8 | 19.5 | 17.1 | 14.7 | 12.3 | 9.8 | 7.2 | 4.7 | 2.1 | -0.5 | -3.1 | -5.7 | -8.2 | -10.8 | -13.3 | -15.7
coeff. [W/V/chord] | 955 | 815 | 723 | 659 | 613 | 579 | 553 | 533 | 519 | 508 | 501 | 496 | 493 | 493 | 495 | 500
S [mm2] | 8527 | 19545 | 20361 | 21207 | 22076 | 22956 | 23835 | 24699 | 25533 | 26323 | 27053 | 27711 | 28285 | 28766 | 29147 | 29426

The slit axis is shifted by to LFS from the chamber axis.

Distance between the slit and the bolometric array is .

Distance between the slit and the plasma centre is .

Spatial resolution of one detector is q = 11 mm

Distance between the chord centre and the plasma centre is given by

Radiated power per given chord (integrated toroidally) is given by

Radiance (power per sr per m2)

Notice:

Positive r means LFS, negative r means HFS.

The channel No.1 is localised at LFS and looks on a part of plasma column at HFS.

The channel No.1 is partially limited by the diagnostic port and is not suitable for a profile reconstruction.

AXUV array 2 (with vertical resolution on plasma column; located at radial flange)

Channel number | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | 16 | 17 | 18 | 19 | 20
r [mm] | 94.1 | 84.5 | 74.6 | 64.6 | 54.4 | 44.1 | 33.6 | 23.0 | 12.4 | 1.7 | -9.0 | -19.6 | -30.2 | -40.7 | -51.2 | -61.4 | -71.5 | -81.4 | -91.1 | -
a [deg] | 16.0 | 14.3 | 12.6 | 10.9 | 9.2 | 7.4 | 5.6 | 3.9 | 2.0 | 0.3 | -1.5 | -3.3 | -5.1 | -6.8 | -8.6 | -10.3 | -12.1 | -13.8 | -15.4 | -
coeff. [W/V /chord] | 731 | 700 | 679 | 663 | 650 | 641 | 633 | 628 | 625 | 624 | 625 | 627 | 632 | 638 | 647 | 658 | 673 | 693 | 720 | -
S [mm2] | 21666 | 21837 | 21992 | 22129 | 22248 | 22348 | 22427 | 22485 | 22521 | 22535 | 22528 | 22498 | 22447 | 22375 | 22282 | 22169 | 22038 | 21888 | 21722 |

The slit axis is not shifted from the chamber axis.

Distance between the slit and the bolometric array is .

Distance between the slit and the plasma centre is .

Spatial resolution of one detector is q = 9 mm

Distance between the chord centre and the plasma centre is given by

Radiated power per given chord (integrated toroidally) is given by

Radiance (power per sr per m2)

Notice:

Positive r means up, negative r means down.

The channel No.1 is localised down and looks on a upper part of plasma column.

The channel No.1 and No.19 are shielded by the diagnostic port and are not suitable for a profile reconstruction.

The channel No.20 is out of order.