Cesky English

Bolometers |
Main | Bolometer | Collecting data & | Output | Measurement &
page | position | Resolution | data | Experiments

Bolometers are used to measure the total radiated power from wide spectral range. Classical pyrobolometers change incident power to the heat. Bolometers present on CASTOR tokamak are silicon photodetectors, which change the radiated power to the electric current. |  |
| When these diodes are exposed to photons of energy greater than 1.12 eV (wavelength less than 1100 nm) electron-hole pairs (carriers) are created. These photogenerated carriers are separated by the p-n junction electric field and a current proportional to the number of electron-hole pairs created flows through an external circuit. For the majority of XUV photons, about 3.7 eV energy is required to generate one electron-hole pair. Thus more than one electron-hole pair is generally created by these photons. This results in device quantum efficiencies (electrons seen by an external circuit per incident photon) much greater than unity, which increase linearly with photon energy. |
Silicon photodiodes AXUV - 20EL were made by International Radiation Detectors Inc. Two unique properties of the AXUV photodiodes provide previously unattainable stable, high quantum efficiencies for XUV photons. The first property is the absence of a surface dead region i.e. no recombination of photogenerated carriers in the doped n-region or at the silicon-silicon dioxide interface. As absorption depths for the majority of XUV photons are less than 1 micrometer in silicon, the absence of a dead region yields complete collection of the photogenerated carriers by an external circuit resulting in 100% carrier collection efficiency and near theoretical quantum efficiency. The second unique property of the AXUV diodes is their extremely thin (3 to 7 nm), radiation-hard silicon dioxide junction passivating, protective entrance window. Owing to these two outstanding properties, the quantum efficiency of AXUV diodes can be approximately predicted in most of the XUV region by the theoretical expression Eph/3.7, where Eph is the photon energy in electron-volts. The only quantum efficiency loss is due to the front (3 to 7 nm) silicon dioxide window at wavelengths for which (mainly for 7 to 100 eV photons) oxide absorption and reflection are not negligible. Owing to their extremely thin (3 to 7 nm) entrance window, AXUV diodes exhibit near theoretical response to low energy electrons and hydrogen ions. Bolometers on CASTOR are two arrays, each with twenty detectors. Detectors have rectangular shape 4 x 0,75 mm and their distance is 0,144 mm. The first array (AXUV 1) has active length 14,16 mm, the second one (AXUV 2) 16,84 mm. |  | up